SCIE Service

Byte

* LIFO
* FIFO

Can a queue be both ?

Short answer Yes !

If you en-act the Conductor….

Html

Get indirectly imply bytes leaving.

Post indirectly imply bytes arriving.

Test Coded April 2022