**Test & Approval**

**Inputs:**

App binaries

How to obtain copy

- Installer msi, zip, web-install

- Dump

- Zip Extracted

**Testbed :**

**Microsoft Windows**

**Testing Terminal Eskom Prepared**

￼

**Model, Theory**

￼

(container framework gateway) EPC, D,R,C

**Present, Tool**

￼

**Deliverables :**

Byte-Array

- SCIE Service read App-Id and Byte-Array from \*.ini file.

List

- Completion run consist of Part-Line[1] and Part-Line[2] thereafter know as Line

Line

- Port-Nat ingress, receive Part-Line[1] to Area ipv4.

- Port-Nat egress, device transmit Part-Line[1] of Device ipv4

- Port-Nat ingress, recieve & reply Part-Line[2] of Device-Host ipv4 (Any Host)

- Port-Nat egress, transmit List[n] to Host ipv4. (Eskom)

Build : Build-Script

Aarch, Lang incremental Versioning

**Kernel**

￼

**Real, Chain**

￼

**Buffer**

￼

**Inter Process Communication**

￼

**Final Target, Deliverable [Build-N]**

**SCIE, (Any)**

￼